**1. PRODUCT and COMPANY IDENTIFICATION**

**Product: Dip Quick Stain Set**

***IN CASE OF EMERGENCY***

***24 HOUR CONTACT TELEPHONE***

***CHEM-TEL: (800)255-3924***

All non-emergency questions may be directed to

customer service (970)669-2500

**Product Code(s):** J-322

**Synonyms:** Mixture

**Manufacturer:** Jorgensen Laboratories, Inc.

1450 North Van Buren Avenue, Loveland, CO 80538

Ph: (970)669-2500 Fax: (970)663-5042

**2. COMPOSITION and INFORMATION on HAZARDOUS INGREDIENTS**

**J-322-1 (#1 – Fixative):**  **Formula % by**

**Ingredients CAS# Formula Weight Hazardous Weight**

Methanol 67-56-1 CH3OH 32.04 Yes >99.9

**J-322-2 (#2 – Eosin) & J-322-3 (#3 – Thiazine): Formula % by**

**Ingredients CAS# Formula Weight Hazardous Weight**

Sodium Azide 26628-22-8 NaN3  65.0 Yes (Raw Material, See Sec 14) 0.01%

**3. HAZARDS IDENTIFICATION**

**J-322-1 (#1 – Fixative):**

**POISON! DANGER! FLAMMABLE! CONTAINS METHANOL! VAPOR HARMFUL. MAY BE FATAL OR CAUSE BLINDNESS IF SWALLOWED. HARMFUL IF INHALED OR ABSORBED THROUGH SKIN. CANNOT BE MADE NONPOISONOUS. FLAMMABLE LIQUID AND VAPOR. CAUSES IRRITATION TO SKIN, EYES, AND RESPIRATORY TRACT. AFFECTS CENTRAL NERVOUS SYSTEM. LIVER AND KIDNEYS.**

**SAFETY RATINGS:** Health: 3, Severe Reactivity: 1, Slight

Flammability: 3, Severe (Flammable) Contact: 3, Severe

**Protective Equipment:** Chemical Safety Glasses/Goggles, Lab Coat/Apron, Gloves, Local/General Ventilation

**Storage Code:** Red: Flammable

**J-322-2 (#2 – Eosin) & J-322-3 (#3 – Thiazine):**

**WARNING! MAY CAUSE IRRITATION TO SKIN, EYES, AND RESPIRATORY TRACT. HARMFUL IF SWALLOWED, INHALED, OR ABSORBED THROUGH SKIN. CONTAINS 0.01% SODIUM AZIDE. SODIUM AZIDE MAY REACT WITH LEAD AND COPPER PLUMBING TO FORM EXPLOSIVE METAL AZIDES.**

**SAFETY RATINGS:** Health: 2, Moderate Reactivity: 1, Slight

Flammability: 0, None Contact: 1, Slight

**Protective Equipment:** Chemical Safety Glasses/Goggles, Lab Coat/Apron, Gloves, Local/General Ventilation

**Storage Code:** Green: General

***Potential Health Effects:***

**J-322-1 (#1 – Fixative):**

**INHALATION:**

A slight irritant to the mucous membranes. Toxic effects exerted upon nervous system, particularly the optic nerve. Once absorbed into the body, it is very slowly eliminated. Symptoms of overexposure may include headache, drowsiness, nausea, vomiting, blurred vision, blindness, coma, and death. A person may get better but then worse again up to 30 hours later.

**INGESTION:**

Toxic! Methyl Alcohol can intoxicate and cause blindness. Usual fatal dose: 100 - 125 milliliters of Methanol. Toxic effects exerted upon nervous system, particularly the optic nerve. Once absorbed into the body, it is very slowly eliminated. Symptoms of overexposure may include headache, drowsiness, nausea, vomiting, blurred vision, blindness, coma, and death.

**SKIN CONTACT:**

Methyl Alcohol is a defatting agent and may cause skin to become dry and cracked. Skin absorption can occur, symptoms may parallel ingestion exposure.

**EYE CONTACT:**

Can cause irritation. Splashes may cause temporary pain and blurred vision. Continued exposure may cause eye lesions.

**POTENTIAL CHRONIC HEALTH EFFECTS:**

Conjunctiva. May cause central nervous system disorder and/or damage. Repeated or prolonged exposure to the substance can produce target organs damage. Marked impairment of vision and enlargement of the liver have been reported. Repeated or prolonged exposure may cause skin irritation.

**MEDICAL CONDITIONS GENERALLY AGGRAVATED by EXPOSURE:**

Persons with pre-existing skin disorders or eye problems or impaired liver or kidney function may be more susceptible to the effects of the substance.

**J-322-2 (#2 – Eosin) & J-322-3 (#3 – Thiazine):**

**INHALATION:**

May cause irritation.

**INGESTION:**

May be harmful or fatal. May cause nausea, vomiting, diarrhea and possible damage to kidneys and thyroid.

**SKIN CONTACT:**

May cause irritation.

**EYE CONTACT:**

May cause irritation.

**POTENTIAL CHRONIC HEALTH EFFECTS:**

No information found.

**MEDICAL CONDITIONS GENERALLY AGGRAVATED by EXPOSURE:**

No information found.

**4. FIRST AID MEASURES**

**J-322-1 (#1 – Fixative):**

**INHALATION:**

Remove to fresh air. If not breathing, give artificial respiration. If breathing is difficult, give oxygen. If symptoms occur, get medical attention.

**INGESTION:**

Induce vomiting immediately as directed by medical personnel. Never give anything by mouth to an unconscious person. Get medical attention immediately.

**SKIN CONTACT:**

Wash with mild soap and water while removing contaminated clothing. If irritation develops, get medical attention.

**EYE CONTACT:**

Check for and remove contact lenses. Immediately flush eyes with gentle but large stream of water for at least 15 minutes, lifting lower and upper eyelids occasionally. If irritation develops, get medical attention.

**J-322-2 (#2 – Eosin) & J-322-3 (#3 – Thiazine):**

**INHALATION:**

Remove to fresh air. If not breathing, give artificial respiration. If breathing is difficult, administer oxygen. If symptoms occur, get medical attention.

**INGESTION:**

Give several glasses of water to drink. Never give anything by mouth to an unconscious person. Get medical attention immediately.

**SKIN CONTACT:**

Wash with mild soap and water while removing contaminated clothing. If irritation develops, get medical attention.

**EYE CONTACT:**

Check for and remove contact lenses. Immediately flush eyes with gentle but large stream of water for at least 15 minutes, lifting lower and upper eyelids occasionally. If irritation develops, get medical attention.

**5. FIRE FIGHTING MEASURES**

**J-322-1 (#1 – Fixative) Methanol:**

**NFPA RATINGS:**  Health: 1 Flammability: 3 Reactivity: 0

**FIRE:**

Flash point: 12oC (54oF) CC  
Autoignition temperature: 464oC (867oF)  
Flammable limits in air % by volume: lel: 6.0, uel: 36  
Flammable Liquid and Vapor!

**EXPLOSION:**

Above flash point, vapor-air mixtures are explosive within flammable limits noted above. Moderate explosion hazard and dangerous fire hazard when exposed to heat, sparks or flames. Sensitive to static discharge.

**FIRE EXTINGUISHING MEDIA:**

Use water, alcohol foam, dry chemical or carbon dioxide.

**SPECIAL INFORMATION:**

In the event of a fire, wear full protective clothing and NIOSH-approved self-contained breathing apparatus with full face piece operated in the pressure demand or other positive pressure mode. Use water spray to blanket fire, cool fire exposed containers, and to flush non-ignited spills or vapors away from fire. Vapors can flow along surfaces to distant ignition source and flash back.

**6. ACCIDENTAL RELEASE MEASURES**

Remove all sources of ignition. Ventilate area of leak or spill. Isolate hazard area and keep unnecessary and unprotected personnel away from the area of the leak or spill. Wear appropriate personal protective equipment as specified in the Exposure Control and Personal Protection Section 8. Use non sparking tools and equipment. Contain and recover liquid when possible. Collect liquid in an appropriate container or absorb with an inert material (e.g. vermiculite, dry sand, earth), and place in a suitable container for reclamation or disposal. Do not use combustible materials, such as sawdust. Do not flush to sewer. US Regulations (CERCLA) require reporting spills and releases to soil, water and air in excess of reportable quantities. The toll free number for the US Coast Guard National Response Center is (800)424-8802.

**7. HANDLING and STORAGE**

Store in a cool, dry, ventilated area away from flame, sources of ignition, heat and incompatible materials. Keep containers tightly closed and upright. Protect from physical damage. Keep out of direct sunlight and separate from incompatible materials. Use non sparking tools and equipment including explosion proof ventilation. When opening metal containers use non-sparking tools because flammable vapors may be present. Containers should be bonded and grounded for transfers to avoid static sparks. Containers of this material may be hazardous when empty since they retain product residues (vapors, liquids); observe all warnings and precautions listed for the product. Storage and use areas should be non-smoking. Wash thoroughly after handling.

**8. EXPOSURE CONTROL and PERSON PROTECTION**

**J-322-1 (#1 – Fixative) Methanol:**

**EXPOSURE LIMITS:**

OSHA: PEL: 200 ppm STEL: 250 ppm TWA: 200 ppm

ACGIH STEL: 250 ppm TWA: 200 ppm

**VENTILATION SYSTEM:**

A system of local and/or general ventilation is recommended to keep employee exposure below airborne limits. Local exhaust ventilation is generally preferred because it can control the emissions of the contaminant at its source, preventing dispersion into the general work area.

**PERSONAL RESPIRATORS (NIOSH) APPROVED:**

If the exposure limit is exceeded and engineering controls are not feasible, wear an appropriate respirator with cartridge for the hazardous material being handled. All respirators should be approved and certified. For emergencies or instances where the exposure levels are not known, use a full face piece positive pressure, air supplied respirator. WARNING: Air purifying respirators do not protect workers in oxygen deficient atmospheres. This substance has poor warning properties.

**SKIN PROTECTION:**

Wear protective clothing, gloves, lab coat or apron, as appropriate, to prevent skin contact.

**EYE PROTECTION:**

Use chemical safety glasses/goggles and/or a full face shield where splashing is possible. Maintain approved eye wash station in work area.

**9. PHYSICAL and CHEMICAL PROPERTIES**

**APPEARANCE:**  **#1, Fixative:** Clear green liquid

**#2, Eosin:** Dark red liquid

**#3, Thiazine:** Dark blue liquid

**ODOR:**  **#1, Fixative:** Characteristic Odor

**#2, Eosin & #3, Thiazine:** Odorless

**SOLUBILITY:** Miscible with water (All)

**SPECIFIC GRAVITY:** No information found

**pH:** No information found

**% VOLATILES by VOLUME:** No information found

**BOILING POINT:** No information found

**MELTING POINT:** No information found

**VAPOR DENSITY (Air =1):** No information found

**VAPOR PRESSURE (mm Hg):** No information found

**EVAPORATION RATE (BuAc=1):** No information found

**10. STABILITY and REACTIVITY**

**J-322-1 (#1 – Fixative):**

**STABILITY:**

Stable under ordinary conditions of use and storage.

**HAZARDOUS DECOMPOSITION PRODUCTS:**

Carbon dioxide, carbon monoxide and formaldehyde may form when heated to decomposition.

**HAZARDOUS POLYMERIZATION:**

Will not occur.

**INCOMPATIBILITIES:**

Strong oxidizing agents such as nitrates, perchlorates or sulfuric acid. Will attack some forms of plastics, rubber, and coatings. May react with metals to generate flammable hydrogen gas.

**CONDITIONS to AVOID:**

Heat, flames, ignition sources and incompatibles.

**J-322-2 (#2 – Eosin) & J-322-3 (#3 – Thiazine):**

**STABILITY:**

Stable under ordinary conditions of use and storage.

**HAZARDOUS DECOMPOSITION PRODUCTS:**

No information found.

**HAZARDOUS POLYMERIZATION:**

Will not occur.

**INCOMPATIBILITIES:**

No information found.

**CONDITIONS to AVOID:**

Heat, flames, ignition sources and incompatibles.

**11. TOXICOLOGICAL INFORMATION**

**J-322-1 (#1 – Fixative) Methanol:**

Oral rat LD50: 5628 mg/kg

Inhalation rat LC50: 64000 ppm/4H

Skin rabbit LD50: 15800 mg/kg

Irritation Data, Standard Draize: Skin rabbit: 20mg/24hr (moderate)

Eye rabbit: 100 mg/24hr (moderate)

Investigated as a tumorigen, mutagen and reproductive effecter.

Cancer Lists --------NTP Carcinogen--------

Ingredient Known Anticipated IARC Category

Methanol (67-56-1) No No None

**12. ECOLOGICAL INFORMATION**

**J-322-1 (#1 – Fixative) Methanol:**

**ENVIROMENTAL FATE:**

When released into the soil, this material may leach into ground water; it is expected to readily biodegrade and quickly evaporates. When released into water, this material is expected to have a half-life between 1 - 10 days. When released into the air, this material is expected to be readily degraded by reaction with photo chemically produced hydroxyl radicals; it is expected to have a half-life between 10 and 30 days. This material is expected to be readily removed from the atmosphere by wet deposition.

**ENVIROMENTAL TOXICITY:**

This material is expected to be slightly toxic to aquatic life.

**13. DISPOSAL INFORMATION**

Whatever cannot be saved for recovery or recycling should be handled as potentially hazardous waste and disposed of or incinerated at an approved waste disposal facility. Processing, use or contamination of this product may change the waste management options. State and local disposal regulations may differ from federal disposal regulations. Dispose of container and unused contents in accordance with federal, state and local requirements.

**14. TRANSPORT INFORMATION**

**J-322-1 (#1 – Fixative):**

**DOT (Land):**

UN1230, Methanol, 3, PG II ERG# 131

**IATA (Air):**

UN1230, Methanol, 3, (6.1), PG II

**IMDG (Sea):**

UN1230, Methanol, 3, PG II ERG: 131

**J-322-2 (#2 – Eosin) & J-322-3 (#3 – Thiazine):**

**DOT (Land), IATA (Air), IMDG (Sea):**

Not regulated.

**15. REGULATORY INFORMATION**

**U.S. FEDERAL REGULATIONS**: Component #1 - Fixative (Methanol) is a "Hazardous Chemical" as defined by the OSHA Hazard Communication Standard, 29 CFR 1910.1200.

Component #1 – Fixative (Methanol) is on the U.S. EPA TSCA Inventory List.

**US EPCRA (SARA Title III) Sections 311/312:**

**Hazard Categories Methanol (#1 – Fixative) #2, #3, Stains**

Section 311 – Hazardous Chemical Yes No

Immediate Hazard Yes No

Delayed Hazard Yes No

Fire Hazard Yes No

Pressure Hazard No No

Reactivity Hazard No No

**US EPCRA (SARA Title III) Section 313 – Toxics Release Inventory:** Methyl Alcohol (67-56-1)

**CERCLA (Superfund) Reportable Quantity:** Methyl Alcohol (67-56-1): 5000 lbs

**CLEAN AIR ACT (CAA):** HAPS list

**INVENTORY STATUS:**

**Methanol (#1 – Fixative)**

**Country(s) or Region Inventory Name On Inventory (Yes/No)\***

Australia Australian Inventory of Chemical Substances (AICS) Yes

Canada Domestic Substances List (DSL) Yes

Canada Non-Domestic Substances List (NDSL) No

China Inventory of Existing Chemical Substances in China (IECSC) Yes

Europe European Inventory of Existing Commercial Chemical Yes

Substances (EINECS)

Europe European List of Notified Chemical Substances (ELINCS) No

Japan Inventory of Existing and New Chemical Substances (ENCS) Yes

Korea Existing Chemicals List (ECL) Yes

New Zealand New Zealand Inventory Yes

Philippines Philippine Inventory of Chemicals and Chemical Substances Yes

(PICCS)

US & Puerto Rico Toxic Substances Control Act (TSCA) Inventory Yes

\*A "Yes" indicates that the listed component(s) of this product comply with the inventory requirements administered by the governing country(s)

**STATE REGULATIONS:**

This product contains 0.01% of Sodium Azide which is known to the State of California to cause cancer, birth defects or other reproductive harm.

**16. OTHER INFORMATION**

**PRODUCT USE:**

For manufacturing, industrial and laboratory use only; not for household use.

**DISCLAIMER:**

Jorgensen Laboratories, Inc. provides the information contained herein in good faith but makes no representation as to its comprehensiveness or accuracy. This document is intended only as a guide to the appropriate precautionary handling of the material by a properly trained person using this product. Individuals receiving the information must exercise their independent judgment in determining its appropriateness for a particular purpose.

JORGENSEN LABORATORIES, INC. MAKES NO REPRESENTATIONS OR WARRANTIES, EITHER EXPRESSED OR IMPLIED, INCLUDING WITHOUT LIMITATION ANY WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE WITH RESPECT TO THE INFORMATION SET FORTH HEREIN OR THE PRODUCT TO WHICH THE INFORMATION REFERS, ACCORDINGLY, JORGENSEN LABORATORIES, INC. WILL NOT BE RESPONSIBLE FOR DAMAGES RESULTING FROM USE OF OR RELIANCE UPON THIS INFORMATION.

REVIEWED 18/2012